{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["12月份采购计划及其他月度采购计划"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"12月份采购计划及其他月度采购计划","index":0,"n_rows":528,"n_cols":10,"rows_kept":528,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["红旗煤矿2024年12月及其他月度材料采购计划"]
["序号","使用单位","标的名称","规格型号","单位","数量","订货要求","单价（元）","总价（元）","计划号"]
[1,"采煤","板梁","0.6*0.12*0.08m","块",400,{"$nulls":3},202412001]
[2,"采煤","道木","0.15*0.15*1.2m","根",200,{"$nulls":3},202412002]
[3,"采煤","润滑脂","长城3#锂基脂 0.001T/代","吨",0.045,{"$nulls":3},202412003]
[4,"采煤","液压支架乳化液","长城牌20—4 0.2T/桶","吨",1.6,{"$nulls":3},202412004]
[5,"采煤","重负荷齿轮油","长城CKD-320# 0.17/桶","吨",0.68,{"$nulls":3},202412005]
[6,"掘一1000、采煤600","铁丝","14#","千克",1600,{"$nulls":3},202412006]
[7,"仓储科","铁丝","11#","吨",20,{"$nulls":3},202412007]
[8,"掘二","背帮","800*80*60mm","根",1000,{"$nulls":3},202412008]
[9,"掘二","背帮","1000*80*60mm","根",1500,{"$nulls":3},202412009]
[10,"掘二","凡士林",null,"瓶",10,{"$nulls":3},202412011]
[11,"掘二","钢带","W型(220*3.75*3300)","根",100,{"$nulls":3},202412012]
[12,"掘二1000、掘一1000","高强锚杆（左旋）","φ20*2400mm                       杆体屈服强度≥500mpa          杆体抗拉强度≥630mpa","套",2000,"含螺母、减磨垫圈、托盘（150*150*10mm）",null,null,202412013]
[13,"掘二","高强锚杆（左旋、镀锌）","φ20*2400mm                       杆体屈服强度≥500mpa           杆体抗拉强度≥630mpa","套",100,"含镀锌螺母、减磨垫圈、镀锌托盘（150*150*10）",null,null,202412014]
[14,"掘二200、掘一100","锚索锁具","φ17.8","个",300,"φ17.8mm锚索配件",null,null,202412016]
[15,"掘二5000、掘一5000","树脂锚固剂","MSCKb2350","支",10000,{"$nulls":3},202412017]
[16,"通巷","红砖","240×115×53mm","块",20000,{"$nulls":3},202412020]
[17,"通巷","木板","4000*250*20mm","块",100,{"$nulls":3},202412021]
[18,"掘一","钢网","2*1","张",600,"开拓巷道 ",null,null,202412022]
[19,"掘一","钢带","W型（220*3.75*3800）","片",200,{"$nulls":3},202412023]
[20,"掘一","钢带","W型（220*3.75*3000）","片",600,{"$nulls":3},202412024]
[21,"掘一","锚索","φ17.8*8000","套",200,"含托盘、锁具（托盘型号：250*250*12）",null,null,202412025]
[22,"运转","锰钢板","10mm","千克",5500,"春节检修",null,null,202412026]
[23,"运转","润滑油","L-HM46#  0.17吨/桶","吨",1.53,"春节检修",null,null,202412027]
[24,"运转","润滑油","L-HM220#  0.17吨/桶","吨",1.87,"春节检修",null,null,202412028]
[25,"运转","锂基酯","长城3#0.015T桶","桶",10,"春节检修",null,null,202412029]
[26,"采煤","擦机布","包皮布白色纯棉10kg/包","公斤",30,{"$nulls":3},202412030]
[27,"采煤","高强防松螺母","M24*2","件",75,"10.9级   细丝",null,null,202412031]
[28,"采煤","高压防水绝缘自粘带","J-20 1KV","盘",30,{"$nulls":3},202412032]
[29,"采煤","高压胶管","KJ3-16×20m /根","根",4,"压力为40Mpa",null,null,202412033]
[30,"采煤","高压胶管","KJ3-25×20m /根","根",4,"压力为35Mpa",null,null,202412034]
[31,"采煤","高压胶管","A51-80-6.5","根",8,{"$nulls":3},202412035]
[32,"采煤","高压胶管","A51-80-2.8","根",8,{"$nulls":3},202412036]
[33,"采煤","螺栓","M20*75（4.8级）","件",200,{"$nulls":3},202412037]
[34,"采煤","煤钻杆","1m/根 方孔（中节）\n两端为母","根",10,{"$nulls":3},202412038]
[35,"采煤","煤钻杆","1m/根 方孔（底节）\n两端为一公一母","根",10,{"$nulls":3},202412039]
[36,"采煤","双针耐震压力表","BZY-60/80Mpa DN10","块",15,{"$nulls":3},202412040]
[37,"采煤","铣把","1.2m","根",40,{"$nulls":3},202412041]
[38,"采煤","铣头","26*34.5cm","张",20,{"$nulls":3},202412042]
[39,"采煤","消防桶","半圆形 铁 枣红 27.5*17*23cm","件",10,{"$nulls":3},202412043]
[40,"采煤","液压球阀","KJ25","件",8,{"$nulls":3},202412044]
[41,"采煤","液压球阀","DN31.5D","件",6,{"$nulls":3},202412045]
[42,"采煤","异径直通","DN31.5D/DN25","件",6,{"$nulls":3},202412046]
[43,"采煤","异径直通","KJ51/DN32","件",6,{"$nulls":3},202412047]
[44,"采煤","U型卡","DN10","件",400,{"$nulls":3},202412048]
[45,"采煤","钢丝编织橡胶护套连接器","SK/conm/4c200cm","根",10,"山东矿机集团公司",null,null,202412049]
[46,"采煤","钢丝编织橡胶护套连接器","SK/conm/4c550cm","根",10,"山东矿机集团公司",null,null,202412050]
[47,"采煤","钢丝编织橡胶护套连接器","SK/conm/4c750cm","根",10,"山东矿机集团公司",null,null,202412051]
[48,"采煤","高压胶管","KJ3-19×1m /根","根",5,"压力为35Mpa",null,null,202412052]
[49,"采煤","注液枪","接口KJ10密封组件材质为铜","把",10,{"$nulls":3},202412053]
[50,"采煤1、掘二2、掘一2","风炮","BK-42","个",5,{"$nulls":3},202412054]
[51,"掘二1、掘一1","手持式气动钻机","ZQS-50/2.5s","台",2,{"$nulls":3},202412055]
[52,"采煤10、掘一20","液压球阀","KJ16","件",30,{"$nulls":3},202412056]
[53,"采煤10/、掘一20","液压球阀","KJ10","件",50,{"$nulls":3},202412057]
[54,"采煤60、掘二20","煤钻头","φ42","个",80,{"$nulls":3},202412058]
[55,"采煤100、掘一100、掘二100","单孔雾化喷头"," 喷雾头 4分 1孔 材质：铜   内丝","件",300,{"$nulls":3},202412059]
[56,"采煤2、掘二4、掘一3","风镐","营口飞亚 G10","个",9,{"$nulls":3},202412060]
[57,"采煤2/掘二10、掘一5","液压球阀","KJ51","件",17,{"$nulls":3},202412061]
[58,"采煤20、、掘一30","聚氨酯阻燃冷补胶","双组分10千克/箱","千克",50,{"$nulls":3},202412062]
[59,"采煤20、掘二30、煤场10、尖锨20","尖铣",null,"张",80,{"$nulls":3},202412063]
[60,"采煤200、掘一500","螺母","M20（4.8级）","件",700,{"$nulls":3},202412064]
[61,"掘一","棉绳","φ6","米",1000,{"$nulls":3},202412065]
[62,"采煤25、掘一50","树脂砂轮切割片","φ400*3.2*32mm","片",75,{"$nulls":3},202412066]
[63,"采煤40、掘二40","变色硅胶","500g/瓶","瓶",80,{"$nulls":3},202412067]
[64,"采煤3000、掘二10000、运输5000、掘一10000","尼龙扎带","φ300*5 白色","根",28000,{"$nulls":3},202412068]
[65,"环保","阀门","SN65","个",1,{"$nulls":3},202412069]
[66,"环保","闸阀","DN100","个",2,"环保喷淋专用",null,null,202412070]
[67,"机厂","螺栓","M8*30","个",200,{"$nulls":3},202412071]
[68,"机厂","螺栓","M8*25","个",200,{"$nulls":3},202412072]
[69,"机厂","轴承",6312,"盘",8,{"$nulls":3},202412075]
[70,"机厂","手把弹簧","Φ2*10*300","根",4,{"$nulls":3},202412076]
[71,"机厂","碳化硅加热板","300*500/2000瓦","个",5,"加热烘烤电机",null,null,202412077]
[72,"机厂","轴承","22222CA","盘",30,"维修减速机",null,null,202412078]
[73,"机厂200、洗煤厂100、掘一60","焊条","φ4.0 J422","千克",360,{"$nulls":3},202412079]
[74,"机厂300、洗煤厂100","焊条","φ3.2 J422","千克",400,{"$nulls":3},202412080]
[75,"掘二","放炮线","GENERAL/通用 放炮线 1米 2×1.5","米",500,{"$nulls":3},202412081]
[76,"掘二","风筒胶","FTJ","瓶",10,{"$nulls":3},202412082]
[77,"掘二50","风钻头","∅32一字","个",50,{"$nulls":3},202412083]
[78,"掘二","风钻头","∅28一字","个",50,{"$nulls":3},202412084]
[79,"掘二","高压胶管","3-51*20m","根",5,{"$nulls":3},202412085]
[80,"掘二","镐锤","一头尖  一头锤  锻打","个",20,{"$nulls":3},202412086]
[81,"掘二","开口滑子（单串铁滑车）","0.5T","个",20,"超速吊梁配件",null,null,202412087]
[82,"掘二","矿用隔爆型电磁阀","DFB20/10 127V","个",2,{"$nulls":3},202412088]
[83,"掘二","螺栓","M16*90","套",200,"（含螺母、平垫、弹簧垫）",null,null,202412089]
[84,"掘二","麻花煤钻杆","φ28*1.6m","个",10,{"$nulls":3},202412090]
[85,"掘二","锚杆连接器","B19钻杆配套","个","30",{"$nulls":3},202412091]
[86,"掘二100、掘一200","锚杆连接套","B19钻杆配套","个","300",{"$nulls":3},202412092]
[87,"掘二","锚索搅拌器","17.8mm-B19","个",10,{"$nulls":3},202412093]
[88,"掘二","煤钻杆","φ38*1.2m","根",20,{"$nulls":3},202412094]
[89,"掘二3、掘一3","喷沙胶管","2SN-φ51*20m  8mpa","根",6,{"$nulls":3},202412095]
[90,"掘二1、掘一1","气动锚杆钻机","MQT-130III型","台",2,"石家庄墨隆",null,null,202412096]
[91,"掘二1、掘一1","气动锚索张拉机具","MQ18-250/65","台",2,{"$nulls":3},202412097]
[92,"掘二1掘一1","气腿式凿岩机","YT28","台",2,"石家庄墨隆",null,null,202412098]
[93,"掘二","绳卡","Φ20 ","个",20,{"$nulls":3},202412099]
[94,"掘二","水炮泥袋","φ50*255","支",10000,{"$nulls":3},202412100]
[95,"掘二","铜喷头","6分内丝φ20","个",100,"单孔雾化",null,null,202412101]
[96,"掘二","温度传感器","GWD95万泰","个",2,{"$nulls":3},202412102]
[97,"掘二","锨把",null,"根",60,{"$nulls":3},202412103]
[98,"掘二700、掘一500","信号电缆","GENERAL/通用 信号电缆 4×1.5   100m/盘","米",1200,{"$nulls":3},202412104]
[99,"掘二","中间接头","KJ10","个",20,{"$nulls":3},202412105]
[100,"掘二50","煤钻头","φ28","个",50,{"$nulls":3},202412106]
[101,"掘二50、掘一50","沟槽式快速接头","DN60  PN6.4Mpa","付",100,"内直径60mm",null,null,202412107]
[102,"掘二20、掘一10、通巷30","液压直通","KJ51","个",60,{"$nulls":3},202412108]
[103,"掘二20、掘一30","风钻杆","B22*1.7m","根",50,{"$nulls":3},202412109]
[104,"掘二20、掘一50","U型卡","KJ51","个",70,{"$nulls":3},202412110]
[105,"掘二20.通巷20","中间接头","KJ16","个",40,{"$nulls":3},202412111]
[106,"掘二300、掘一500、","螺栓","M20*75(4.8级）","套",800,"（含螺母、平垫、弹簧垫）",null,null,202412112]
[107,"掘二","锚杆钻杆","B19*1m","根","50",{"$nulls":3},202412113]
[108,"掘二50、掘一30","绳卡","Φ8","个",80,{"$nulls":3},202412114]
[109,"掘二50、掘一30","液压直通","KJ10","个",80,{"$nulls":3},202412115]
[110,"掘二50、掘一40","锚杆钻头（金刚石钻头）","LONGGONG/龙工 自选金刚石复合片钻头 28# ","个",90,{"$nulls":3},202412116]
[111,"掘二500、掘一600","U型卡","KJ10","个",1100,{"$nulls":3},202412117]
[112,"掘二60、掘一30","煤铣","26*34.5cm","张",90,{"$nulls":3},202412118]
[113,"掘二60、掘一40","风镐钎子","500mm","根",100,{"$nulls":3},202412119]
[114,"掘一","309装饰胶",null,"千克",5,{"$nulls":3},202412120]
[115,"掘一","u型卡","KJ25","个",200,{"$nulls":3},202412121]
[116,"掘一","安全带","涤纶、带护腰及缓冲器","条",2,{"$nulls":3},202412122]
[117,"掘一","白漆","调和漆：白漆 15kg/桶","公斤",60,{"$nulls":3},202412123]
[118,"掘一","编织袋","96*55","条",200,{"$nulls":3},202412124]
[119,"掘一","草绿漆","调和漆：绿漆 15kg/桶","公斤",30,{"$nulls":3},202412125]
[120,"掘一","穿条","φ8*800","根",30,{"$nulls":3},202412126]
[121,"掘一","大红漆","调和漆：大红漆 15kg/桶","公斤",30,{"$nulls":3},202412127]
[122,"掘一","单串铁滑车","0.5T","个",10,{"$nulls":3},202412128]
[123,"掘一","凡士林","医用","瓶",10,{"$nulls":3},202412129]
[124,"掘一","防爆两联按钮","36v ","台",2,{"$nulls":3},202412130]
[125,"掘一","高压防水自粘带","J--20  1Kv","盘",10,{"$nulls":3},202412131]
[126,"掘一","机布","白色 纯棉 10kg/包 ","公斤",50,{"$nulls":3},202412132]
[127,"掘一","卡箍式快速接头","DN108 PN6.4MPa","付",50,{"$nulls":3},202412133]
[128,"掘一","矿用电缆钩","φ58","个",400,{"$nulls":3},202412134]
[129,"掘一","矿用电缆冷补模具","FCS3-1.5","个",10,{"$nulls":3},202412135]
[130,"掘一","锂基脂","2#、1kg/袋","袋",60,{"$nulls":3},202412136]
[131,"掘一","螺栓","M16*75-8.8级","套",100,"含弹垫、螺母",null,null,202412137]
[132,"掘一","螺栓","M16*50-4.8级","套",300,"含弹垫、螺母",null,null,202412138]
[133,"掘一","锚杆搅拌器","32mm--B19","个",20,{"$nulls":3},202412139]
[134,"掘一","锚杆拉力计","LDZ--400","台",2,{"$nulls":3},202412140]
[135,"掘一","煤钻杆","Φ28*2.2m（带丝)","个",30,"钻头与钻杆连接方式：上丝",null,null,202412141]
[136,"掘一","煤钻杆","Φ28*1.6m（带丝)","个",20,"钻头与钻杆连接方式：上丝",null,null,202412142]
[137,"掘一","耐震压力表","0--60Ma","个",10,{"$nulls":3},202412143]
[138,"掘一","扭力扳手","180-760N.s","把",1,{"$nulls":3},202412144]
[139,"掘一","皮带扣","GORO-RV6-800mm","盒",10,{"$nulls":3},202412145]
[140,"掘一","射钉枪","NS307S","个",1,"南山牌",null,null,202412146]
[141,"掘一","射钉枪子弹","S3-6.8*1.8","盒",10,"南山牌",null,null,202412147]
[142,"掘一","声光语音信号","KXH127v","台",4,{"$nulls":3},202412148]
[143,"掘一","铣把",null,"根",50,{"$nulls":3},202412149]
[144,"掘一","鱼尾螺栓","φ20*90","套",200,{"$nulls":3},202412150]
[145,"掘一","轴承","22312CA","个",10,{"$nulls":3},202412151]
[146,"掘一","混凝土钢模板","400mm*1200mm","块",30,{"$nulls":3},202412152]
[147,"掘一","混凝土钢模板","200mm*1200mm","块",30,{"$nulls":3},202412153]
[148,"掘一","螺栓","φ20*80(4.8级）","套",100,{"$nulls":3},202412154]
[149,"掘一","锚杆压力载荷压力表","MC2--300","个",20,"支架用",null,null,202412155]
[150,"掘一10、掘二10","注水器","内丝φ16","个",20,"与φ28煤钻杆配套使用",null,null,202412156]
[151,"掘一","自喷漆（白色）",null,"瓶",12,{"$nulls":3},202412157]
[152,"掘一150、运转100","稀释剂（稀料）",null,"公斤",250,{"$nulls":3},202412158]
[153,"煤场","阀门","DN100 PN16 HT200","个",4,{"$nulls":3},202412159]
[154,"煤场","平铣","平","个",10,"包括铣把",null,null,202412160]
[155,"煤场","消防卡箍","65mm","个",20,{"$nulls":3},202412161]
[156,"煤场4/洗煤厂10","消防水带","16-65-25含接头+喷枪","套",14,{"$nulls":3},202412162]
[157,"通防","负压风筒","500mm*10m","节",6,{"$nulls":3},202412163]
[158,"通防","机械秒表","MA","个",3," 井下测风用",null,null,202412164]
[159,"通防","矿用阻燃剂","MEA防火材料 20kg/袋","吨",1,"提供安全性和环保性评估报告、产品批次合格证",null,null,202412165]
[160,"通防","束管接头","10mm不锈钢接头防锈处理","个",50,{"$nulls":3},202412166]
[161,"通防","微色谱束管","10mm不锈钢接头防锈处理","米",3000,"淄博祥龙KSS-200D微微色谱专用",null,null,202412167]
[162,"通防","微色谱载气","8L/He（99.999%）","瓶",3,"淄博祥龙KSS-200D微色谱专用瓶（有空瓶）",null,null,202412168]
[163,"通防","微色谱9组分标气","H2、O2、N2、CO、CO2、CH4、C2H2、C2H4、C2H6","瓶",3,"急，淄博祥龙KSS-200D微色谱专用瓶",null,null,202412169]
[164,"通防","矿用计算器MA","MA","个",3," 井下测风用",null,null,202412170]
[165,"通防","气体采样袋","1L单阀铝箔","个",50,{"$nulls":3},202412171]
[166,"通巷"," O型圈"," Φ16","个",100,{"$nulls":3},202412172]
[167,"通巷","编织袋 ","50*80cm","条",2000,{"$nulls":3},202412173]
[168,"通巷","单滑轮"," 304不锈钢 M25","个",200,{"$nulls":3},202412174]
[169,"通巷","地质钻杆","Φ50mm*1m","根",300,"不要小加工厂代加工钻杆、丝头容易断裂，报废率高",null,null,202412175]
[170,"通巷","电池"," 南孚1号 1.5V","节",40,{"$nulls":3},202412176]
[171,"通巷","钢丝绳卡子"," Φ8","个",100,{"$nulls":3},202412177]
[172,"通巷","球形截止阀","KJ16","个",50,{"$nulls":3},202412178]
[173,"通巷","法兰式金属软管 ","DN80*2m PN6.4Mpa   不锈钢国标法兰","根",2,{"$nulls":3},202412179]
[174,"通巷100、运转30","生料带"," 王中王","盘",130,{"$nulls":3},202412180]
[175,"通巷24、掘一24","自喷漆"," 红色 400ml/瓶","瓶",48,{"$nulls":3},202412181]
[176,"洗煤厂","电焊钳","DL23880 500-1000A","个",5,{"$nulls":3},202412182]
[177,"洗煤厂","高亮LED灯泡","36w","个",30,{"$nulls":3},202412183]
[178,"洗煤厂","割枪","2#","把",5,{"$nulls":3},202412184]
[179,"洗煤厂","哈夫节补漏器","DN200*400","个",20,{"$nulls":3},202412185]
[180,"洗煤厂","金属切割片","100*16*2.5mm","个",100,{"$nulls":3},202412186]
[181,"洗煤厂","聚丙烯酰胺","阴离子","吨",2,{"$nulls":3},202412187]
[182,"洗煤厂","锂基脂","1#/15KG","千克",10,{"$nulls":3},202412188]
[183,"洗煤厂","煤铣","3#","个",20,{"$nulls":3},202412189]
[184,"洗煤厂","尼龙棒（白色）","φ20","米",10,{"$nulls":3},202412190]
[185,"洗煤厂","尼龙棒（白色）","φ30","米",10,{"$nulls":3},202412191]
[186,"洗煤厂","氧气表","DL-YQY","块",3,{"$nulls":3},202412192]
[187,"洗煤厂","乙炔表"," DL-YQE","块",3,{"$nulls":3},202412193]
[188,"运输","PU软管 ","φ12*8mm","米",200,{"$nulls":3},202412194]
[189,"运输","道夹板","φ22kg（国标）","付",100,{"$nulls":3},202412195]
[190,"运输","防爆接线盒","BHD2-40A-3G","个",2,{"$nulls":3},202412196]
[191,"运输","手动扳道器","φ30kg","台",6,{"$nulls":3},202412197]
[192,"运输","信号电缆","MYQ4*1.5","米",200,{"$nulls":3},202412198]
[193,"通巷75、掘一90","调合漆","天蓝15kg /桶","千克",165,{"$nulls":3},202412199]
[194,"运转","53件套棘轮螺丝批套装","世达05491","套","2","设备维修使用",null,null,202412200]
[195,"运转","ATOS放大器","E-MI-AC-OIF20/2ATOS","个",1,"主副井绞车维修",null,null,202412201]
[196,"运转","YX型密封圈轴用","D28×34×8","个",10,{"$nulls":3},202412202]
[197,"运转","不锈钢球阀","DN20","个",10,{"$nulls":3},202412203]
[198,"运转","不锈钢球阀","DN25","个",10,{"$nulls":3},202412204]
[199,"运转","不锈钢球阀","DN32 ","个",5,{"$nulls":3},202412205]
[200,"运转","大喷壶","1500ml","个",4,"质量标准化用",null,null,202412206]
[201,"运转","弹簧式安全阀","AK28W-16T DN25 压力范围0.7-1.0介质：空气\n整定压力0.93 MPa 工作压力0.85MPA","个",3,"主副井绞车维修",null,null,202412207]
[202,"运转","弹性胶圈","24×45×45","个",60,{"$nulls":3},202412208]
[203,"运转","电动对夹蝶阀","690D97A1X3P-10 DN100 DRT-10 380V 北京鼎瑞特阀门有限公司","个","4","污水处理站用",null,null,202412209]
[204,"运转","吊顶一体钉","M8吊顶专用钉","盒",3,{"$nulls":3},202412210]
[205,"运转","调和漆","灰色15KG/桶","千克",90,"质量标准化用",null,null,202412211]
[206,"运转","调和漆","桔红色15KG/桶","千克",60,"质量标准化用",null,null,202412212]
[207,"运转","调和漆","蓝色15KG/桶","千克",120,"质量标准化用",null,null,202412213]
[208,"运转","法兰闸阀","Z41T-16 DN100 HT200 1.6MPa 明杆","个",2,{"$nulls":3},202412214]
[209,"运转","风机启动电容","ABB Arcotronics 1.27.4AA2 MKP 6uF±5% ","个","4","通风机房",null,null,202412215]
[210,"运转","高压胶管","∲51   20M","根",1,{"$nulls":3},202412216]
[211,"运转","高压胶管","∲51   10M","根",2,{"$nulls":3},202412217]
[212,"运转","高压熔断器","RN2-10  10KV 0.5A","个",12,"35kv变电所",null,null,202412218]
[213,"运转","高压验电笔","GDY-Ⅱ10KV","个",2,"35kv变电所",null,null,202412219]
[214,"运转","隔绝式压缩氧自救器","ZYX30","个",50,{"$nulls":3},202412220]
[215,"运转","光电传感器","NI15-M30-AP6X","个",20,"主副井绞车",null,null,202412221]
[216,"运转","焊接弯头","φ108（加厚1.5倍）","个",20,{"$nulls":3},202412222]
[217,"运转","搅拌机","BLD10-17-1.5KW电机型号YE3-90L-4常州凯常威电机（轴套杆+单片三叶片）","套",1,"污水处理",null,null,202412223]
[218,"运转","就地控制箱","450*350*160mmm、304不锈钢、一启动、一停止、一绿色指示灯、一红色指示灯。装配1.德力西DZ47-100A断路器1个。2.德力西CJX2S-6511 65A交流接触器1个。3.德力西TGR36-63热过载继电器1个。220V","套","3",{"$nulls":3},202412224]
[219,"运转","麻花钻头","12×125","个",10,"设备维修",null,null,202412225]
[220,"运转","耐震压力表","YN-100  1MPA径向","块",6,"主副井绞车",null,null,202412226]
[221,"运转","耐震压力表","YN-100  0-6MPA径向","块",6,"主副井绞车",null,null,202412227]
[222,"运转","盘式盒装安全警戒带","5cm*2mm 50m/盒 警戒线字样 帆布","盒","4",{"$nulls":3},202412228]
[223,"运转","平垫圈"," M12  4.8","个",1000,{"$nulls":3},202412229]
[224,"运转","球阀","KJ10","个",10,{"$nulls":3},202412230]
[225,"运转","球阀","KJ25","个",10,{"$nulls":3},202412231]
[226,"运转","球阀","KJ16","个",10,{"$nulls":3},202412232]
[227,"运转","射钉","M8×65","盒",10,{"$nulls":3},202412233]
[228,"运转","消防阀门","DN65","个","6","地面消防设施维修用",null,null,202412234]
[229,"运转","真空压力表","Y-100-0.1MPA","块",6,"主副井绞车",null,null,202412235]
[230,"运转","指示灯","AD16-16E  AC/DC24v红色","个",10,"主副井绞车",null,null,202412236]
[231,"运转","指示灯","AD16-16E  AC/DC24v绿色","个",10,"主副井绞车",null,null,202412237]
[232,"运转","铸造缺陷修补剂","K-9110 AB胶 500g/套 卡夫特","套",2,"设备维修",null,null,202412238]
[233,"运转","时间继电器","SS-22/1  100V","个",5,"主副井维修",null,null,202412239]
[234,"运转","时间继电器","DV-24C   100V","个",5,"主副井维修",null,null,202412240]
[235,"运转","角铁","80×80（6米/根）","千克",1600,"皮带用",null,null,202412241]
[236,"运转","断路器","DZ47S-63 3P 63A 380V","个",10,"各岗点维修使用",null,null,202412242]
[237,"运转","断路器","DZ47-60(DZ47-63) 2P 32A","个",10,"各岗点维修使用",null,null,202412243]
[238,"运转","高压绝缘手套","2级带电作业用I型最大使用电压10000V","双",4,"变电所用",null,null,202412244]
[239,"运转","金属石墨线垫片","DN200B型","个",5,"接管用",null,null,202412245]
[240,"运转","无缝钢管","∲121无缝钢管（6米/根）","千克",150,"深部用",null,null,202412246]
[241,"运转","沟槽弯头","110沟槽","个",20,{"$nulls":3},202412247]
[242,"运转","O型圈","10×2.6","个",50,{"$nulls":3},202412248]
[243,"运转","O型圈","16×2.8","个",50,{"$nulls":3},202412249]
[244,"运转","O型圈","25×3.3","个",50,{"$nulls":3},202412250]
[245,"运转","O型圈","50×3.6","个",50,{"$nulls":3},202412251]
[246,"运转","沟槽卡箍","φ165","个",10,{"$nulls":3},202412252]
[247,"运转","涡轮对夹蝶阀","D371X-10/16手动齿轮转动碟阀水阀12寸DN150","个",2,"污水处理站",null,null,202412253]
[248,"运转","塑壳断路器","CKM33-200H 200A","个","2","压风机房",null,null,202412254]
[249,"运转","矿用位置传感器","GUC100  DC24V","个",2,"主副绞车维修",null,null,202412255]
[250,"运转","三相多功能仪表","CD194E-354","个",3,"主副绞车维修",null,null,202412256]
[251,"运转","三相多功能仪表","CD194E-254","个",3,"主副绞车维修",null,null,202412257]
[252,"运转","YX型密封圈","D70×82×14","个",10,"开关用",null,null,202412258]
[253,"运转","YX型密封圈","D130×142×14","个",10,{"$nulls":3},202412259]
[254,"运转","YX型密封圈","D125×137×14","个",10,{"$nulls":3},202412260]
[255,"运转","法兰盘","∲159孔中心距24CM","个",10,"焊管用",null,null,202412261]
[256,"运转","煤油",null,"公斤",50,"春节检修",null,null,202412262]
[257,"运转","超强投光灯","GT9100 Φ580*555mm 1000W","个",10,"矿上照明",null,null,202412263]
[258,"运转","手动涡轮对夹式蝶阀","D371X-10/16Q  DN350","个","4","污水处理站",null,null,202412264]
[259,"运转","百分表","表头+表座","个",1,"主副绞车维修",null,null,202412265]
[260,"运转","高压接地棒","25mm²线3×1米+1×5米","个",2,"深部变电所",null,null,202412266]
[261,"运转60、掘一30","调和漆","黄色15KG/桶","千克",90,"质量标准化用",null,null,202412267]
[262,"运转90、掘一30 ","调和漆","黑色15KG/桶","千克",120,"质量标准化用",null,null,202412268]
[263,"总务","LED射灯"," 2.5寸嵌入式 内径6.5cm","个",20,{"$nulls":3},202412269]
[264,"总务","PVC磨砂帘子","长2600mm 宽200mm\n厚2mm","片",100,{"$nulls":3},202412270]
[265,"总务","大脚踏延时冲洗阀","1寸6706","个",10,{"$nulls":3},202412271]
[266,"总务","电工绝缘胶带","PVC黑色","盘",20,{"$nulls":3},202412272]
[267,"总务","海尔暖风机","金色机械款HN2201\n8cm*16cm*74cm","台",5,"海尔牌",null,null,202412273]
[268,"总务","卷纸（厕纸）","110mm*100mm  10卷/提","提",10,"清风牌",null,null,202412274]
[269,"总务","垃圾袋小33#   ","黑色 100卷/袋\n33*52cm","袋",10,"厚实的",null,null,202412275]
[270,"总务","生料带","水暖件专用","盘",30,{"$nulls":3},202412276]
[271,"总务","小笤帚","高粱苗","把",100,{"$nulls":3},202412277]
[272,"总务","低噪音轴流通风机","304不锈钢 SFG5-4\n功率750W 电压380V 转速1450 外径56cm 内径51cm 防水耐磨","个",5,"澡堂散热用",null,null,202412278]
[273,"总务","面盆水龙头","单孔 单冷","个",20,{"$nulls":3},202412279]
[274,"总务","PPR球阀","32活节","个",10,{"$nulls":3},202412280]
[275,"总务","自动香薰机","壁挂式 安装5号电池\n（每套带精油5瓶）\n105*105*39mm","套",2,{"$nulls":3},202412281]
[276,"总务","化工泵","220V 流量4M³/小时\n长41cm宽19.5cm高35cm\n接头内径32*25MM\n接头外径38*32MM","台",1,"澡堂用",null,null,202412282]
[277,"总务","耙子","不锈钢 长155cm草耙子","把",10,{"$nulls":3},202412283]
[278,"调度室","矿用语音声光风门开闭状态传感器","GFK30(A)","个","5",{"$nulls":3},202412284]
[279,"调度室","PVC电气胶带","24mm","盘",20,"固定光缆接线处用",null,null,202412285]
[280,"调度室","矿用通讯电缆","MHYAV1*6*7*0.37","米","2000","井下用设备电缆",null,null,202412286]
[281,"调度室","矿用本质安全型烟雾传感器","GQQ5(A)","台","5","江苏三恒\n通讯设备电缆",null,null,202412287]
[282,"调度室","矿用阻燃网线","MHYVP4*2*1/0.97","米","2000","井下用设备网线",null,null,202412288]
[283,"调度室","尼龙扎带","200*4 白色","根",10000,"设备吊挂用",null,null,202412289]
[284,"调度室","矿用机电设备开停传感器","KTT9-D","个",6,"风机开停用",null,null,202412290]
[285,"调度室","煤矿用通信光缆","MT/T386-2011 MGTSV-8B","米",1000,"井上下视频安装及连接监控分站、无线基站使用",null,null,202412291]
[286,"调度室","矿用铠装单模光纤跳线","4芯 LC-LC（小头） 5米","根","20","优普连\n井下用设备光纤",null,null,202412292]
[287,"生活科","LED灯","海德信LED BPZ4200-T140   40W","个",5,"海德信",null,null,202412293]
[288,"生活科","净水器阻垢剂",null,"桶",1,"净化水用",null,null,202412294]
[289,"仓储科","插排","六位总控1.5米","个",3,"办公室使用",null,null,202412295]
[290,"采煤","半滚筒","1LB01-2","件",1,{"$nulls":3},202412296]
[291,"采煤","拨链器","代号S40T0106A","件",4,{"$nulls":3},202412297]
[292,"采煤","阀体组件","BRW250.03.04","件",5,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412298]
[293,"采煤","钢套组件","BRW200.03.02","件",5,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412299]
[294,"采煤","隔圈","BRW200.03.02-4","件",60,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412300]
[295,"采煤","刮板链","3GL03 (1.28米/挂）","挂",75,{"$nulls":3},202412301]
[296,"采煤","滑块密封","BRW250.03.06","件",5,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412302]
[297,"采煤","截齿","U47 （含卡簧）","件",40,"无锡科菲",null,null,202412303]
[298,"采煤","截齿套","U85 （含卡簧）","件",120,"无锡科菲",null,null,202412304]
[299,"采煤","链轮","1LB01-1","件",2,{"$nulls":3},202412305]
[300,"采煤","液力耦合器","YOXD450A（ 含梅花垫）","件",1,{"$nulls":3},202412306]
[301,"采煤","一轴总成","SZB630/75转载机用","件",2,{"$nulls":3},202412307]
[302,"采煤","主控器","TX458","件",1,"无锡科菲",null,null,202412308]
[303,"采煤","柱塞（050）","BRW200.0301-1","件",10,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412309]
[304,"采煤","自动卸载阀","XF400II","件",1,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412310]
[305,"采煤","柱塞密封圈","BRW200.03.02-5","件",60,"BRW315/31.5乳化泵（南京六合鼎扬制泵有限公司）",null,null,202412311]
[306,"采煤","弹性块","2DLPD201-5","件",6,{"$nulls":3},202412312]
[307,"采煤","连接环","3GL01 -2","件",50,{"$nulls":3},202412313]
[308,"采煤","刮板","3GL01 -3","件",30,"刮板机用",null,null,202412314]
[309,"采煤","盲轴总成","7S06/010107","件",1,{"$nulls":3},202412315]
[310,"采煤1、掘二2","轴皮半滚筒","SGB620/40T输送机用","件",3,{"$nulls":3},202412316]
[311,"采煤2、掘一3","液力耦合器","YOXD400 （ 含弹性套）","件",5,{"$nulls":3},202412317]
[312,"采煤6、掘一8","机头压链器","SGB620/40T  2个为一付","件",14,{"$nulls":3},202412318]
[313,"仓储科","成型套","SA-105","个",8,"编网机用",null,null,202412319]
[314,"仓储科","绕丝板","SA-109","个",8,{"$nulls":3},202412320]
[315,"仓储科","校正套","SA-106","个",8,{"$nulls":3},202412321]
[316,"仓储科","剪切大臂","SA-DB","套",1,{"$nulls":3},202412322]
[317,"机厂","电机风叶","φ75","个",10,{"$nulls":3},202412323]
[318,"机厂","电机风叶","φ65","个",10,{"$nulls":3},202412324]
[319,"机厂","漆包线","φ1.06","千克",100,{"$nulls":3},202412325]
[320,"机厂","漆包线","φ1.25","千克",100,{"$nulls":3},202412326]
[321,"机厂","尾轮壳","40T","件",3,{"$nulls":3},202412327]
[322,"机厂","电机风叶","φ132","个",10,"维修电机",null,null,202412328]
[323,"机厂","隔爆型电力液压鼓式制动器","YWZ4-300/45，电压660/1140（焦作市起重控制电器）","台",2,"维修皮带机",null,null,202412329]
[324,"机厂","矿车轮端盖","高度450mm，盖缘厚度5mm，盖缘外径120mm（厂家:凤台中煤亚太矿山机械制造有限公司）","个",40,"维修矿车",null,null,202412330]
[325,"机厂","电机后端盖","YBK3-200L2-6（无锡安利达电机）","件",2,"维修电机",null,null,202412331]
[326,"掘二","锚索张拉千斤顶","适配φ17.8mm*8m锚索","个",2,{"$nulls":3},202412332]
[327,"掘二","喷头总成","51喷砂管用","件",5,"喷浆机配件",null,null,202412333]
[328,"掘二","压链器","40T 2个/付","付",6,{"$nulls":3},202412334]
[329,"掘二10、掘一10、采煤6","分链器","40T刮板输送机配件","个",26,{"$nulls":3},202412335]
[330,"掘二6、掘一6","小架子","40T刮板输送机配件","件",12,{"$nulls":3},202412336]
[331,"掘二30、掘一30、采煤30","弹性套","SGB-40T","件",90,{"$nulls":3},202412337]
[332,"掘一","盲轴总成","40T刮板输送机配件","件",2,{"$nulls":3},202412338]
[333,"掘一","机尾滚筒总成","40T刮板输送机配件","个",4,{"$nulls":3},202412339]
[334,"掘一4","舌板","SGB-40T刮板输送机配件","个",4,{"$nulls":3},202412340]
[335,"掘二50、掘一20","对轮销子","SGB-40T","个",70,{"$nulls":3},202412341]
[336,"掘二6、掘一6、采煤2","链轮","40T刮板输送机配件","件",14,{"$nulls":3},202412342]
[337,"掘一","分链器销子","40T","个",20,{"$nulls":3},202412343]
[338,"掘一","喷浆机喷头","PZ--5喷浆机用（不带座）","个",6,{"$nulls":3},202412344]
[339,"掘一","张拉千斤顶","φ17.8","个",2,{"$nulls":3},202412345]
[340,"掘一","张拉千斤顶","φ22","个",2,{"$nulls":3},202412346]
[341,"掘一","轴皮半滚筒","40T","付",2,{"$nulls":3},202412347]
[342,"煤场","轮胎（三角）","23.5-25","个",4,"含护毂胎",null,null,202412348]
[343,"通巷","气体自动负压采样器","CFZ20","台",2,{"$nulls":3},202412349]
[344,"通巷","手推车","翻斗960*580*410mm 高750mm 总宽800mm 双轮 实心轮","辆",1,{"$nulls":3},202412350]
[345,"洗煤厂","跳汰机筛板","孔径φ16mm，长59.5cm×宽108cm×高5cm\n","块",12,{"$nulls":3},202412351]
[346,"洗煤厂","跳汰机筛板","孔径φ13mm，长59.5cm×宽108cm×高5cm\n","块",12,{"$nulls":3},202412352]
[347,"洗煤厂","脱水筛筛板","660mm×587mm*50mm","块",10,{"$nulls":3},202412353]
[348,"洗煤厂","压滤机控制屏","6av6 648-OBC11-3AX0 山东德州京津环保科技公司","个",1,"需要装入程序运行",null,null,202412354]
[349,"洗煤厂","跳汰机控制屏","skt-10","个",1,"需要装入程序运行",null,null,202412355]
[350,"洗煤厂","托辊","全长2750mm，直径90mm,托辊长2500mm，两头扁20mm,端头13mm","个",100,"皮带用",null,null,202412356]
[351,"洗煤厂","跳汰机变频器","skt-10","个",2,"需要装入程序运行",null,null,202412357]
[352,"洗煤厂","压滤机变频器","SIEMENS-SinamicsV20","个",1,"需要装入程序运行",null,null,202412358]
[353,"运输","刹车总成","5T","套",4,"电瓶车用",null,null,202412359]
[354,"运输","照明综保插件","ZBZ-2.5/4M","件",5,{"$nulls":3},202412360]
[355,"运转","弹性圆柱销","12×90","个",1000,"井下皮带维修用",null,null,202412361]
[356,"运转","弹性柱销","M20×24×105","个",20,"井下皮带维修用",null,null,202412362]
[357,"运转","电磁换向阀","DKE-1711DC10","个",3,"副井口上下液压站",null,null,202412363]
[358,"运转","电磁换向阀","DBHI-0631","个",3,"副井口上下液压站",null,null,202412364]
[359,"运转","电磁换向阀","DBHI-0711","个",3,"副井口上下液压站",null,null,202412365]
[360,"运转","电磁换向阀","DBHI-0713","个",3,"副井口上下液压站",null,null,202412366]
[361,"运转","防爆磁性接近开关","KSC1010A-1/22","台",4,"主副井绞车",null,null,202412367]
[362,"运转","给煤机减速机总成","GLD800/5.5/S型甲带式给料机驱动轮（加齿轮）380/660","个",1,"给煤机",null,null,202412368]
[363,"运转","开关柜智能操控装置","ZK3-077Y AK-ZK6300 编号10101592 安科电气","个",4,"主副井绞车",null,null,202412369]
[364,"运转","开关柜智能操控装置","ZK3-308R AK-ZK6300 编号10030205 安科电气","个","6","主副井绞车",null,null,202412370]
[365,"运转","开关柜智能操控装置","ZK3-314R AK-ZK6300 编号10030221 安科电气","个","2","主副井绞车",null,null,202412371]
[366,"运转","开关柜智能操控装置","ZK3-312R AK-ZK6300 编号10030222 安科电气","个",2,"主副井绞车",null,null,202412372]
[367,"运转","梅花垫","295×160×50×10（急用）","个",10,"井上下皮带",null,null,202412373]
[368,"运转","盘型制动器","TS223中信重工","副",2,"春节检修",null,null,202412374]
[369,"运转","盘型制动器","TS222中信重工","副",2,"春节检修",null,null,202412375]
[370,"运转","罐笼链子","4×2","米",300,"副井口",null,null,202412376]
[371,"运转","热保护器","MT—63/3H厂家LS电气","个",5,"热泵防",null,null,202412377]
[372,"运转","网络摄像头","DS-3T35D/i5 含支架电源 主机厂家：海康威视","个","10","通风机房",null,null,202412378]
[373,"运转","光端机","RS485光端机 A.B端 威博科技","套",2,"通风机房",null,null,202412379]
[374,"运转","梅花垫","MT2（68×28×18）6角","个",10,"井上下皮带维修",null,null,202412380]
[375,"运转","电磁接触器","MC—65a厂家LS电气","个",5,"主副井维修",null,null,202412381]
[376,"运转","振动传感器","GBD20矿用本安型振动传感器   徐州致拓自动化有限公司","个","2","通风机房",null,null,202412382]
[377,"生活科","切菜机配件刀片（切丁）","XK280多功能切菜机","组",1,{"$nulls":3},202412383]
[378,"生活科","切菜机配件刀片（切丝）","XK280多功能切菜机","个",1,{"$nulls":3},202412384]
[379,"生活科","切菜机配件（皮带）","XK280多功能切菜机","条",1,{"$nulls":3},202412385]
[380,"生活科","切菜机配件（电机）","XK280多功能切菜机","个",1,{"$nulls":3},202412386]
[381,"生活科","配电柜交流接触器","CJ20-100","个",2,{"$nulls":3},202412387]
[382,"机厂","矿工钢","20mnk  10米/根","kg",30000,"支护材料",null,null,202412388]
[383,"机厂","槽钢","12#  ","kg",1000,"支护材料",null,null,202412389]
[384,"调度室","煤矿用高浓度激光甲烷传感器","GJG100J","台","1","江苏三恒\n监测监控设备",null,null,202412390]
[385,"调度室","矿用本安型读卡器","KJ1150-D3","套","10","重庆梅安森\n人员定位设备",null,null,202412391]
[386,"调度室","矿用本安型基站","KJ787-F1","台",5,"重庆梅安森\n人员定位设备",null,null,202412392]
[387,"调度室","矿用多路隔爆兼本安型直流稳压电源","KDW660-24B(B)","台","3","重庆梅安森\n人员定位电源",null,null,202412393]
[388,"调度室","矿用本安型监控分站","KJ770-F5（A)","台",5,"江苏三恒监测监控控制设备断电使用",null,null,202412394]
[389,"调度室","矿用多路隔爆兼本安型直流稳压电源","KD660-24BJ","台","5","江苏三恒监测监控控制设备断电使用",null,null,202412395]
[390,"调度室","矿用本安型IP网络广播终端","KXT23.1","台","3","天地常州\n语音通讯联络",null,null,202412396]
[391,"调度室","煤矿用一氧化碳传感器","GTH1000","个",5,"江苏三恒\n监测监控设备",null,null,202412397]
[392,"调度室","矿用隔爆兼本安型断电器","KDG1140（A)","台","6","监测监控控制设备断电使用",null,null,202412398]
[393,"调度室","煤矿用风筒风量开关传感器","GFD6（A）","台",2,"监测监控设备",null,null,202412399]
[394,"机电运输科","照明综保开关","ZBZ-16-4.0","台",6,"电光、深部",null,null,202412400]
[395,"机电运输科","真空馈电开关","KBZ-16-400","台",10,"电光、深部",null,null,202412401]
[396,"机电运输科","真空电磁开关","QJZ-16-120","台",5,"电光、备用",null,null,202412402]
[397,"机电运输科","真空电磁开关","QJZ-16-60N","台",5,"电光、备用",null,null,202412403]
[398,"机电运输科","真空电磁开关","QJZ-16-30","台",7,"电光、备用",null,null,202412404]
[399,"通巷","煤矿用深孔钻车","CMS1-1200/45(Z)   履带式深孔钻机整机+配件（详见备注）","套",1,"配件明细：配套钻杆42*1m*200根、65钻头10个、扶正器1套、扩孔器1套",null,null,202412405]
[400,"通巷","矿用气动阻化泵","BZQ-40/2.5","台",1,{"$nulls":3},202412406]
[401,"运转","直流电机","DC48-200W正联机电（厂家）","台",1,"罐笼帘用",null,null,202412407]
[402,"运转","清水离心泵","DFW200-250N4  22KW380V 上海东方泵业有限公司","台","1","污水处理站",null,null,202412408]
[403,"运转","电动高压无气喷涂机","工业级 电动喷涂机6000（双枪） 藤原","台","1","质量标准化",null,null,202412409]
[404,"运转","海康威视硬盘录像机","DS-8608N-K2  带两块8T硬盘","台","1","通风机房及矿灯房",null,null,202412410]
[405,"运转","减速机","RVO50/15正联机电（厂家）","台",1,"皮带用",null,null,202412411]
[406,"运转","转臂行星摩擦无级变速机","MB75YB75×W6   7.5kw  380/660","个",1,"地面给煤机",null,null,202412412]
[407,"运转","柱栓泵","210RSO4.5DR/3K-PPA-13Y100","台",1,"副井液压站用",null,null,202412413]
[408,"运转","立式管道离心泵","ISG150-315A 上海创科泵业制造有限公司22KW电机380V","台","1","污水处理站",null,null,202412414]
[409,"通巷","快速喷涂材料","PT PU·SixOy(F)（每套两罐共20kg）","套",20,"优先选择山西凝固力新型材料股份有限公司产品",null,null,"专项事项审批单"]
[410,"运转","矿用隔爆型永磁式高压真空配电装置（显示）","高防开关显示：与保护器PA63—NBA配套显示：因泰莱","个",1,"井下高防开关使用",null,null,202407032]
[411,"洗煤厂","高频调速三相异步电动机","4kw 唐山汇力科技有限公司","台",1,{"$nulls":3},202407158]
[412,"洗煤厂","不锈钢焊条","A102","千克",20,"焊接筛板",null,null,202408101]
[413,"运转","石笔","68*9*4.2","盒",20,"设备维修划线使用",null,null,202408142]
[414,"总务科","灭火器箱","53*45*19 容4KG*2灭火器  \n201材质","个",2,"洗衣房及男澡堂放置灭火器使用",null,null,202408168]
[415,"采煤","耳轴",null,"件",20,"3191工作面ZF6800/17/32支架用",null,null,202408267]
[416,"采煤","数字压力计","YHY60（D）（带支杆）","块",1,"3191工作面单体支柱测压用",null,null,202411088]
[417,"采煤","单体支柱测压仪","SY-40 （带压力杆）","块",1,"3191工作面单体支柱测压用",null,null,202411089]
[418,"掘一","镀锌扁铁","40*6000mm","根",6,{"$nulls":3},202411097]
[419,"运转","异形扁铁","7*7  6米/根","根","5","主副井设备维修使用",null,null,202411256]
[420,"机厂","焊锡丝","含锡50% φ1.0mm","卷",10,"维修电器",null,null,202411303]
[421,"机厂","花键套","液力耦合器YOXD 400 弹性套式","个",10,"河南省华升矿机    修液力耦合器",null,null,202411332]
[422,"调度室","可调温电烙铁","数显内热 150W","个",1,"维修电器设备",null,null,202411361]
[423,"总务科","防滑垫","绿色6mm  宽1.2米","米",50,"澡堂地面防滑使用",null,null,202411398]
[424,"总务科","可裁剪丝圈                 防滑地垫","绿色 厚15mm 宽1.5米            18米/卷","卷",2,"公共场所台阶防滑使用",null,null,202411399]
[425,"总务科","工业盐","50斤/袋","袋",40,"冬季防滑防冻使用",null,null,202411404]
[426,"采煤","柱塞密封圈","BRW200.03.02-5","件",50,"3191工作面BRW315/31.5乳化泵用（南京六合鼎扬制泵有限公司）",null,null,202411416]
[427,"采煤","滑块密封","BRW250.03.06","件",5,"3191工作面BRW315/31.5乳化泵用（南京六合鼎扬制泵有限公司）",null,null,202411417]
[428,"采煤","弹性块","2DLPD201-5","件",6,"3191工作面PLM500型轮式破碎机用 （山东矿机）",null,null,202411420]
[429,"采煤","阀体组件","BRW250.03.04","件",5,"3191工作面BRW315/31.5乳化泵用（南京六合鼎扬制泵有限公司）",null,null,202411424]
[430,"采煤","卸载阀","XF400","件",2,"3191工作面BRW315/31.5乳化泵用（南京六合鼎扬制泵有限公司）",null,null,202411425]
[431,"采煤","阀座","HHDYFZDN10","件",20,"3191工作面电液控阀组材质为PEEK(山东矿机）",null,null,202411433]
[432,"采煤","阀座","HHDYFZDN20","件",20,"3191工作面电液控阀组材质为PEEK(山东矿机）",null,null,202411434]
[433,"运转","柱栓泵","L10VS045DR/3R-PPA-13N00","台","1","副井液压站泵头使用",null,null,202411474]
[434,"运转","不锈钢加强型喉箍抱箍管夹卡子","40mm-43mm.48mm-51mm.52mm-55mm","各",5,"地面各设备维修使用",null,null,202411485]
[435,"机厂","接线室","40千瓦电机，喇叭口φ72mm","个",2,"山防电机 维修电机",null,null,202411525]
[436,"机厂","接线室","40千瓦电机，喇叭口φ90mm","个",2,"南阳电机 维修电机",null,null,202411526]
[437,"通巷工区","钻套","钻机机头/钻杆连接套      \n","个",6,"钻机型号ZQJC730/10.7主机厂家邹城兖矿泰德工贸有限公司。井下防灭火探钻使用",null,null,202411550]
[438,"调度室","功率开关管","XNG100B24TC1S5-100A","只",10,"维修电器设备",null,null,202411551]
[439,"调度室","功率开关管","K1120 1000v ","只",10,"维修电器设备",null,null,202411553]
[440,"调度室","二极管","DSA90C200HB","只",10,"维修电器设备",null,null,202411554]
[441,"调度室","二极管","MBRF30100CT ","只",10,"维修电器设备",null,null,202411555]
[442,"调度室","电阻","杂散电阻 1/2W","包",1,"维修电器设备",null,null,202411564]
[443,"运转","溜槽","原煤机头至振动筛（异型）高3、5mx1、2mx1、2m含导料槽","个",1,{"$nulls":3},202411583]
[444,"机电科","环氧树脂冷浇铸剂","G—20","盒",30,"32深部变电所",null,null,202411673]
[445,"机电科","高爆开关导电杆绝缘座","内孔m20 高压开关PJG315/10Y用","个",30,"32深部变电所",null,null,202411674]
[446,"机电科","高爆开关导电杆绝缘小座","内孔m20 高压开关PJG315/10Y用","个",30,"32深部变电所",null,null,202411675]
[447,"机电科","高爆开关手动合闸操作机构"," 高压开关PJG315/10Y用","个",2,"32深部变电所",null,null,202411676]
[448,"机电科","镀锌扁铁","宽40x4(mm)","根","100","32深部变电所",null,null,202411681]
[449,"机电科","高爆开关负荷侧喇叭口","配高压开关PJG315/10Y用","个",5,"32深部变电所",null,null,202411682]
[450,"机电科","矿用隔爆型高压接线盒（铠装电缆）","小型设备","台","4",{"$nulls":3},202411699]
[451,"掘二","温度传感器","GWH100天津华宁","个",2,{"$nulls":3},202411195]
[452,"掘二","雷管箱","300*200*250mm","个",2,{"$nulls":3},202411236]
[453,"掘二","锂电充电式电动扳手","博世GDS250-LI双锂电18V","把",1,"锚杆钻机维修工具",null,null,202411237]
[454,"掘二","耙装机照明灯","36v","个",2,{"$nulls":3},202411245]
[455,"运输","电解液","浓度1.26-1.28","千克",2000,{"$nulls":3},202411278]
[456,"洗煤厂","哈夫节补漏器密封垫","DN200*400","个",20,{"$nulls":3},202411336]
[457,"运转","连接小车","TBC6—342.1-0203","节","4","副井操车大修用",null,null,202411473]
[458,"运转","阀门控制器 ","控制箱 220vac 开关盒电动蝶阀控制器调试盒","个",2,"热泵供洗澡水使用",null,null,202411481]
[459,"运转","板式球阀","QJH—10B","个",2,"主井车房液压站使用",null,null,202411487]
[460,"运转","光端机","（RS485光端机）A.B端 威博科技","套",1,"通风机房电柜维修使用",null,null,202411490]
[461,"运输","矿用本安型闪光\n红尾灯","DHY3.7L","个",4,{"$nulls":3},202411491]
[462,"机厂","滚筒壳","Φ320*950","件",2,"维修皮带机",null,null,202411498]
[463,"调度室","功率热敏电阻","NTC5D-11","只",10,"维修电器设备",null,null,202411565]
[464,"运转","立式单级离心泵","100KQL94-70-30/2 30KW 上海凯泉泵业有限公司","台",1,{"$nulls":3},202411586]
[465,"运转","  污水排污泵","80WQ60—40—15KW    上海东方泵业有限公司","台",1,{"$nulls":3},202411587]
[466,"机电科","矿用隔爆型照明信号综合保护装置","ZBZ16-10/1140（660）（1140V变660V)","台",2,{"$nulls":3},202411669]
[467,"机电科","红外温度传感器","GWH100（A）","台",2,"35深部绞车房",null,null,202411672]
[468,"掘一","单串铁滑车","0.5T","个",10,{"$nulls":3},202411107]
[469,"掘二","元钉","50mm","千克",50,{"$nulls":3},202411155]
[470,"掘二","棉绳","φ6","公斤",100,{"$nulls":3},202411164]
[471,"掘二","开关保护盒","WZBQ-1型微机磁力启动器保护装置（中国 电光）","个",4,{"$nulls":3},202411249]
[472,"运转","压槽机铜套","30*34*40","个",10,"风水管路维修使用",null,null,202411263]
[473,"运转","膨胀管芯","M8*100","个",50,"风水管路维修使用",null,null,202411270]
[474,"运转","烟雾探测器测试剂",null,"瓶",10,"设备维修使用",null,null,202411271]
[475,"运转","聚合氯化铝","30% 黄色 粉末状 喷雾式","吨",10,"污水站污水处理使用",null,null,202411272]
[476,"运转","聚丙烯酰胺","阴离子 2000万分子量以上","吨",2,"污水站污水处理使用",null,null,202411273]
[477,"运输","蒸馏水","25kg/桶\n济宁市恒业化验用品有限公司","千克",1000,{"$nulls":3},202411279]
[478,"运输","起重链条连接器","H型5/8（适用于16-20mm链条）","个",20,{"$nulls":3},202411287]
[479,"运输","继电器","JZX-22F/4Z（D）","个",10,"翻矸机配件",null,null,202411290]
[480,"机厂","扁平吊装带","3T*3m","条",2,"吊装",null,null,202411298]
[481,"机厂","稀释剂","20千克/桶 奔腾","桶",2,"复新",null,null,202411302]
[482,"机厂","O型圈","410*6","个",20,"修液力耦合器",null,null,202411333]
[483,"机厂","O型圈","290*6","个",20,"修液力耦合器",null,null,202411334]
[484,"洗煤厂","纯牛油盘根填料绳","16mm×16mm","KG",10,{"$nulls":3},202411341]
[485,"通巷工区","元钉","80mm","千克",100,"井下构筑临时控风设施及日常使用",null,null,202411350]
[486,"通巷工区","高压油管快速接头","丝扣39×2  ","套",2,"ZDY-1900钻机油管连接快速接头",null,null,202411352]
[487,"通巷工区","高压油管快速接头","丝扣30×1.5 ","套",6,"ZDY-1900钻机油管连接快速接头",null,null,202411353]
[488,"通巷工区","高压油管快速接头","丝扣32×1.5  ","套",6,"ZDY-1900钻机油管连接快速接头",null,null,202411354]
[489,"总务科","PPR双活接铜球阀热熔管阀门","25型","个",10,"维修澡堂管道使用",null,null,202411378]
[490,"总务科","换气扇","体积260mm*115mm*235mm\n功率25W 规格：180mm 玻璃窗式","个",2,"办公场所卫生间使用",null,null,202411396]
[491,"总务科","管道疏通机弹簧","16mm","盘",1,"疏通下水道使用",null,null,202411397]
[492,"总务科","保温皮帘子","200cm*60cm 2片\n280cm*100cm 4片\n280cm*248cm 2片\n(颜色棕红色，已附图片)","片",8,"澡堂门口保暖使用",null,null,202411402]
[493,"仓储科","线切割液","DX-2","公斤",360,{"$nulls":3},202411411]
[494,"采煤","隔圈","BRW200.03.02-4","件",50,"3191工作面BRW315/31.5乳化泵用（南京六合鼎扬制泵有限公司）",null,null,202411415]
[495,"采煤","挡圈","34.9*32.1*0.8","件",50,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411437]
[496,"采煤","挡圈","33.9*31.1*0.8","件",50,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411438]
[497,"采煤","挡圈","21.5*18.2*0.8","件",50,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411439]
[498,"采煤","挡圈","12.9*9.5*0.8","件",100,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411440]
[499,"采煤","挡圈","19.9*16.5*0.8","件",100,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411441]
[500,"采煤","挡圈","30.9*28.1*0.8","件",50,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411442]
[501,"采煤","挡圈","29.9*27.1*0.8","件",100,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411443]
[502,"采煤","挡圈","16.5*13.1*0.8","件",100,"3191工作面电液控阀组用材质为聚甲醛",null,null,202411444]
[503,"运输","圆环链条","18*64mm","米",30,"爬车机配件",null,null,202411495]
[504,"机厂","真空接触器","CKJ5-400 电压1140V 电流400A 控制电压AC36V","件",3,"维修开关",null,null,202411519]
[505,"机厂","转子","4kw水泵 轴径30mm转子长33.5cm 叶轮直径25mm 定子长24.7cm","件",2,"淮南大通 维修水泵",null,null,202411520]
[506,"机厂","转子","5.5kw水泵 轴径30mm 转子长37cm 叶轮直径25mm 铁芯长142*97","件",2,"淮南大通 维修水泵",null,null,202411521]
[507,"机厂","喇叭口","φ72mm","个",3,"山防电机 维修电机",null,null,202411522]
[508,"机厂","喇叭口","φ90mm","个",3,"南阳电机 维修电机",null,null,202411523]
[509,"机厂","电机风叶","轴径φ65mm","件",6,"维修电机",null,null,202411524]
[510,"机厂","信号照明本体","ZBZ-4.0","件",2,"电光防爆 维修照明综保",null,null,202411529]
[511,"机厂","交流接触器","CJT1-20A 127V德力西","个",8,"维修照明综保",null,null,202411530]
[512,"机厂","先导接触器","HHC70A1-2Z JT-2C DC12V","个",15,"维修照明综保",null,null,202411531]
[513,"机厂","按钮控制","BZA1-5-36-3","个",30,"维修三联按钮",null,null,202411532]
[514,"调度室","功率开关管","FGA60N65SMD-650V","只",10,"维修电器设备",null,null,202411552]
[515,"调度室","开关电源控制IC","TNY279PN ","只",10,"维修电器设备",null,null,202411556]
[516,"调度室","开关电源控制IC","VIPer22A ","只",10,"维修电器设备",null,null,202411557]
[517,"调度室","开关电源控制IC","TOP256YN ","只",10,"维修电器设备",null,null,202411558]
[518,"调度室","电阻","RXG24 2K/10W      ","只",10,"维修电器设备",null,null,202411562]
[519,"调度室","电阻","RXG24 10K/10W","只",10,"维修电器设备",null,null,202411563]
[520,"洗煤厂","聚丙烯酰胺 ","阴离子","吨",2,{"$nulls":3},202411573]
[521,"机电科","矿用电缆固定S钩","大开口25","个",400,{"$nulls":3},202411641]
[522,"机电科","槽型托辊"," D=108","个",100,{"$nulls":3},202411656]
[523,"机电科","摩擦调心托辊架"," D=108","个",10,{"$nulls":3},202411657]
[524,"机电科","上调心托辊",null,"组",10,{"$nulls":3},202411658]
[525,"机电科","摩擦下调心托辊架","图纸编号DT‖03C2823","个",10,{"$nulls":3},202411659]
[526,"机电科","下调心托辊",null,"组",10,{"$nulls":3},202411660]